-------------------------------------------------------------------------- 

       511121-44 MOBILTRANS HD 10W
          MATERIAL SAFETY DATA BULLETIN
-------------------------------------------------------------------------- 

-------------------------------------------------------------------------- 
1. PRODUCT AND COMPANY IDENTIFICATION
-------------------------------------------------------------------------- 
PRODUCT NAME: MOBILTRANS HD 10W
SUPPLIER: EXXONMOBIL OIL CORPORATION
          3225 GALLOWS RD.
          FAIRFAX,  VA   22037

24 - Hour Health and Safety Emergency (call collect):  609-737-4411

24 - Hour Transportation Emergency:
CHEMTREC: 800-424-9300   202-483-7616
LUBES AND FUELS: 281-834-3296

Product and Technical Information:
Lubricants and Specialties:  800-662-4525   800-443-9966
Fuels Products:  800-947-9147
MSDS Fax on Demand: 713-613-3661
MSDS on Internet: http://www.exxon.com
                  http://www.mobil.com

-------------------------------------------------------------------------- 
2. COMPOSITION/INFORMATION ON INGREDIENTS
-------------------------------------------------------------------------- 
CHEMICAL NAMES AND SYNONYMS: PET. HYDROCARBONS AND ADDITIVES

GLOBALLY REPORTABLE MSDS INGREDIENTS:

  Substance Name           Approx. Wt%
  --------------           -----------
  ALKYL PHENYL ETHER            <1

OTHER INGREDIENTS:

  Substance Name           Approx. Wt%
  --------------           -----------
  ZINC ARYLDITHIOPHOSPHATE        1-5

  SULFONIC ACIDS, PETROLEUM,      1-5
   CALCIUM SALTS, OVERBASED
   (68783-96-0)

See Section  8 for exposure limits (if applicable).

-------------------------------------------------------------------------- 
3. HAZARDS IDENTIFICATION
-------------------------------------------------------------------------- 
Under normal conditions of use, this product is not considered hazardous
according to regulatory guidelines (See section 15).

EMERGENCY OVERVIEW: Brown Liquid.  DOT ERG No. :  NA

POTENTIAL HEALTH EFFECTS: Under normal conditions of intended use, this
     product does not pose a risk to health.  Excessive exposure may
     result in eye, skin or respiratory irritation.

POTENTIAL ENVIRONMENTAL EFFECTS: Harmful to aquatic organisms, may cause
     long-term adverse effects in the aquatic environment.

For further health effects/toxicological data, see Section 11.

-------------------------------------------------------------------------- 
4. FIRST AID MEASURES
-------------------------------------------------------------------------- 
EYE CONTACT: Flush thoroughly with water.  If irritation occurs, call a
     physician.
SKIN CONTACT: Wash contact areas with soap and water.  Remove and clean
     oil soaked clothing daily and wash affected area.  (See Section 16 -
     Injection Injury)
INHALATION: Not expected to be a problem.  However, if respiratory
     irritation, dizziness, nausea, or unconsciousness occurs due to
     excessive vapor or mist exposure, seek immediate medical assistance.
     If breathing has stopped, assist ventilation with a mechanical
     device or mouth-to-mouth resuscitation.
INGESTION: Not expected to be a problem.  Seek medical attention if
     discomfort occurs.  Do not induce vomiting.

-------------------------------------------------------------------------- 
5. FIRE-FIGHTING MEASURES
-------------------------------------------------------------------------- 
EXTINGUISHING MEDIA: Carbon dioxide, foam, dry chemical and water fog.
SPECIAL FIRE FIGHTING PROCEDURES: Water or foam may cause frothing.  Use
     water to keep fire exposed containers cool.  Water spray may be used
     to flush spills away from exposure.  Prevent runoff from fire
     control or dilution from entering streams, sewers, or drinking water
     supply.
SPECIAL PROTECTIVE EQUIPMENT: For fires in enclosed areas, fire fighters
     must use self-contained breathing apparatus.
UNUSUAL FIRE AND EXPLOSION HAZARDS: None.
COMBUSTION PRODUCTS: Fumes, smoke, carbon monoxide, sulfur oxides,
     aldehydes and other decomposition products, in the case of
     incomplete combustion.
Flash Point C(F): 202(396) (ASTM D-92).
Flammable Limits (approx.% vol.in air) -   LEL:  0.9%,   UEL:  7.0%
NFPA HAZARD ID:   Health: 0,  Flammability: 1,  Reactivity: 0

-------------------------------------------------------------------------- 
6. ACCIDENTAL RELEASE MEASURES
-------------------------------------------------------------------------- 
NOTIFICATION PROCEDURES: Report spills/releases as required to
     appropriate authorities.  U.S. Coast Guard and EPA regulations
     require immediate reporting of spills/releases that could reach any
     waterway including intermittent dry creeks.  Report spill/release to
     Coast Guard National Response Center toll free number (800)424-8802.
     In case of accident or road spill notify CHEMTREC (800) 424-9300.
PROCEDURES IF MATERIAL IS RELEASED OR SPILLED:
     LAND SPILL: Shut off source taking normal safety precautions.  Take
     measures to minimize the effects on ground water.  Recover by
     pumping or contain spilled material with sand or other suitable
     absorbent and remove mechanically into containers.  If necessary,
     dispose of adsorbed residues as directed in Section 13.
     WATER SPILL: Confine the spill immediately with booms.  Warn other
     ships in the vicinity.  Notify port and other relevant authorities.
     Remove from the surface by skimming or with suitable absorbents.  If
     permitted by regulatory authorities the use of suitable dispersants
     should be considered where recommended in local oil spill
     procedures.
ENVIRONMENTAL PRECAUTIONS: Prevent material from entering sewers, water
     sources or low lying areas; advise the relevant authorities if it
     has, or if it contaminates soil/vegetation.
PERSONAL PRECAUTIONS: See Section 8

-------------------------------------------------------------------------- 
7. HANDLING AND STORAGE
-------------------------------------------------------------------------- 
HANDLING: No special precautions are necessary beyond normal good hygiene
     practices.  See Section 8 for additional personal protection advice
     when handling this product.
STORAGE: Keep containers closed when not in use.  Do not store in open or
     unlabelled containers.  Store away from strong oxidizing agents and
     combustible materials.  Do not store near heat, sparks, flame or
     strong oxidants.
SPECIAL PRECAUTIONS: Prevent small spills and leakages to avoid slip
     hazard.
EMPTY CONTAINER WARNING: Empty containers retain residue (liquid and/or
     vapor) and can be dangerous. DO NOT PRESSURIZE, CUT, WELD, BRAZE,
     SOLDER, DRILL, GRIND OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME,
     SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION; THEY MAY
     EXPLODE AND CAUSE INJURY OR DEATH. Do not attempt to refill or clean
     container since residue is difficult to remove. Empty drums should
     be completely drained, properly bunged and promptly returned to a
     drum reconditioner. All containers should be disposed of in an
     environmentally safe manner and in accordance with governmental
     regulations.

-------------------------------------------------------------------------- 
8. EXPOSURE CONTROLS/PERSONAL PROTECTION
-------------------------------------------------------------------------- 

OCCUPATIONAL EXPOSURE LIMITS:

When mists/aerosols can occur, the following are recommended:  5 mg/m3
(as oil mist)- ACGIH Threshold Limit Value (TLV), 10 mg/m3 (as oil mist)
- ACGIH Short Term Exposure Limit (STEL), 5 mg/m3 (as oil mist) - OSHA
Permissible Exposure Limit (PEL)

VENTILATION: If mists are generated, use adequate ventilation, local
     exhaust or enclosures to control below exposure limits.
RESPIRATORY PROTECTION: If mists are generated, and/or when ventilation
     is not adequate, wear approved respirator.
EYE PROTECTION: If eye contact is likely, safety glasses with side
     shields or chemical type goggles should be worn.
SKIN PROTECTION: Not normally required.  When splashing or liquid contact
     can occur frequently, wear oil resistant gloves and/or other
     protective clothing.  Good personal hygiene practices should always
     be followed.

-------------------------------------------------------------------------- 
9. PHYSICAL AND CHEMICAL PROPERTIES
-------------------------------------------------------------------------- 
Typical physical properties are given below.  Consult Product Data Sheet
for specific details.

APPEARANCE: Liquid
COLOR: Brown
ODOR: Mild
ODOR THRESHOLD-ppm: NE
pH: NA
BOILING POINT C(F): > 316(600)
MELTING POINT C(F): NA
FLASH POINT C(F): 202(396) (ASTM D-92)
FLAMMABILITY (solids): NE
AUTO FLAMMABILITY C(F): NA
EXPLOSIVE PROPERTIES: NA
OXIDIZING PROPERTIES: NA
VAPOR PRESSURE-mmHg 20 C: < 0.1
VAPOR DENSITY: > 2.0
EVAPORATION RATE: NE
RELATIVE DENSITY, 15/4 C: 0.888
SOLUBILITY IN WATER: Negligible
PARTITION COEFFICIENT: > 3.5
VISCOSITY AT 40 C, cSt:   42.0
VISCOSITY AT 100 C, cSt:   6.3
POUR POINT C(F): -33(-27)
FREEZING POINT C(F): NE
VOLATILE ORGANIC COMPOUND: NE
DMSO EXTRACT, IP-346 (WT.%): <3, for mineral oil only
            NA=NOT APPLICABLE NE=NOT ESTABLISHED D=DECOMPOSES

FOR FURTHER TECHNICAL INFORMATION, CONTACT YOUR MARKETING REPRESENTATIVE

-------------------------------------------------------------------------- 
10. STABILITY AND REACTIVITY
-------------------------------------------------------------------------- 
STABILITY (THERMAL, LIGHT, ETC.): Stable.
CONDITIONS TO AVOID: Extreme heat and high energy sources of ignition.
INCOMPATIBILITY (MATERIALS TO AVOID): Strong oxidizers.
HAZARDOUS DECOMPOSITION PRODUCTS: Product does not decompose at ambient
     temperatures.
HAZARDOUS POLYMERIZATION: Will not occur.

-------------------------------------------------------------------------- 
11. TOXICOLOGICAL DATA
-------------------------------------------------------------------------- 
                         ---ACUTE TOXICOLOGY---
ORAL TOXICITY (RATS):  Practically non-toxic (LD50:  greater than 2000
     mg/kg).  ---Based on testing of similar products and/or the
     components.
DERMAL TOXICITY (RABBITS):  Practically non-toxic (LD50:  greater than
     2000 mg/kg).  ---Based on testing of similar products and/or the
     components.
INHALATION TOXICITY (RATS):  Practically non-toxic (LC50:  greater than 5
     mg/l).  ---Based on testing of similar products and/or the
     components.
EYE IRRITATION (RABBITS):  Practically non-irritating.  (Draize score:
     greater than 6 but 15 or less).  ---Based on testing of similar
     products and/or the components.
SKIN IRRITATION (RABBITS):  Practically non-irritating.  (Primary
     Irritation Index:  greater than 0.5 but less than 3).  ---Based on
     testing of similar products and/or the components.
OTHER ACUTE TOXICITY DATA: Although an acute inhalation study was not
     performed with this product, a variety of mineral and synthetic
     oils, such as those in this product, have been tested.  These
     samples had virtually no effect other than a nonspecific
     inflammatory response in the lung to the aerosolized mineral oil.
     The presence of additives in other tested formulations (in
     approximately the same amounts as in the present formulation) did
     not alter the observed effects.

                  ---SUBCHRONIC TOXICOLOGY (SUMMARY)---
No significant adverse effects were found in studies using repeated
     dermal applications of similar formulations to the skin of
     laboratory animals for 13 weeks at doses significantly higher than
     those expected during normal industrial exposure.  The animals were
     evaluated extensively for effects of exposure (hematology, serum
     chemistry, urinalysis, organ weights, microscopic examination of
     tissues etc.).

                 ---REPRODUCTIVE TOXICOLOGY (SUMMARY)---
No teratogenic effects would be expected from dermal exposure, based on
     laboratory developmental toxicity studies of major components in
     this formulation and/or materials of similar composition.

                   ---CHRONIC TOXICOLOGY (SUMMARY)---
Repeated and/or prolonged exposure may cause irritation to the skin, eyes
     or respiratory tract.  Overexposure to oil mist may result in oil
     droplet deposition and/or granuloma formation.  For mineral base
     oils:  Base oils in this product are severely solvent refined and/or
     severely hydrotreated.  Chronic mouse skin painting studies of
     severely treated oils showed no evidence of carcinogenic effects.
     These results are confirmed on a continuing basis using various
     screening methods such as Modified Ames Test, IP-346, and/or other
     analytical methods.  For synthetic base oils:  The base oils in this
     product have been tested in the Ames assay and other tests of
     mutagenicity with negative results.  These base oils are not
     expected to be carcinogenic with chronic dermal exposures.

                      ---SENSITIZATION (SUMMARY)---
Not expected to be sensitizing based on tests of this product,
     components, or similar products.

-------------------------------------------------------------------------- 
12. ECOLOGICAL INFORMATION
-------------------------------------------------------------------------- 

ENVIRONMENTAL FATE AND EFFECTS:

This environmental assessment was conducted using information on the
     individual components as no test data was available for this
     specific formulation.

ECOTOXICITY: This product is expected to be harmful to aquatic organisms.
     May cause long-term adverse effects in the aquatic environment.

MOBILITY: When released into the environment, adsorption to sediment and
     soil will be the predominant behavior.

PERSISTENCE AND DEGRADABILITY: This product is expected to be inherently
     biodegradable.

BIOACCUMULATIVE POTENTIAL: Bioaccumulation is unlikely due to the very
     low water solubility of this product, therefore bioavailability to
     aquatic organisms is minimal.

-------------------------------------------------------------------------- 
13. DISPOSAL CONSIDERATIONS
-------------------------------------------------------------------------- 
WASTE DISPOSAL: Product is suitable for burning in an enclosed,
     controlled burner for fuel value.  Such burning may be limited
     pursuant to the Resource Conservation and Recovery Act.  In
     addition, the product is suitable for processing by an approved
     recycling facility or can be disposed of at an appropriate
     government waste disposal facility.  Use of these methods is subject
     to user compliance with applicable laws and regulations and
     consideration of product characteristics at time of disposal.

RCRA INFORMATION:  The unused product, in our opinion, is not
     specifically listed by the EPA as a hazardous waste (40 CFR,
     Part 261D), nor is it formulated to contain materials which
     are listed hazardous wastes.  It does not exhibit the hazardous
     characteristics of ignitability, corrosivity, or reactivity. The
     unused product is not formulated with substances covered by the
     Toxicity Characteristic Leaching Procedure (TCLP).  However, used
     product may be regulated.

-------------------------------------------------------------------------- 
14. TRANSPORT INFORMATION
-------------------------------------------------------------------------- 
USA DOT:  NOT REGULATED BY USA DOT.

RID/ADR:  NOT REGULATED BY RID/ADR.

IMO:  NOT REGULATED BY IMO.

IATA:  NOT REGULATED BY IATA.

STATIC ACCUMULATOR (50 picosiemens or less):  YES

-------------------------------------------------------------------------- 
15. REGULATORY INFORMATION
-------------------------------------------------------------------------- 

US OSHA HAZARD COMMUNICATION STANDARD: When used for its intended
     purposes, this product is not classified as hazardous in accordance
     with OSHA 29 CFR 1910.1200.

EU Labeling: Product is dangerous as defined by the European Union
     Dangerous Substances/Preparations Directives.

  Symbol: Not applicable.

  Risk Phrase(s): R52/53.
     Harmful to aquatic organisms, may cause long-term adverse effects in
     the aquatic environment.

  Safety Phrase(s): S61.
     Avoid release to the environment.  Refer to special
     instructions/Safety data sheets.

Governmental Inventory Status: All components comply with TSCA,
     EINECS/ELINCS, AICS, METI, DSL, KOREA, and PHILIPPINES.

U.S. Superfund Amendments and Reauthorization Act (SARA) Title III:
  This product contains no "EXTREMELY HAZARDOUS SUBSTANCES".

  SARA (311/312) REPORTABLE HAZARD CATEGORIES: None.

  This product contains no chemicals subject to the supplier notification
  requirements of SARA (313) toxic release program.

The following product ingredients are cited on the lists below:
CHEMICAL NAME                         CAS NUMBER     LIST CITATIONS * 
-------------                         ----------     --------------
ZINC (ELEMENTAL ANALYSIS)  (0.13%)     7440-66-6     22

                    --- REGULATORY LISTS SEARCHED ---
1=ACGIH ALL  6=IARC 1     11=TSCA 4    16=CA P65 CARC   21=LA RTK
2=ACGIH A1   7=IARC 2A    12=TSCA 5a2  17=CA P65 REPRO  22=MI 293
3=ACGIH A2   8=IARC 2B    13=TSCA 5e   18=CA RTK        23=MN RTK
4=NTP CARC   9=OSHA CARC  14=TSCA 6    19=FL RTK        24=NJ RTK
5=NTP SUS   10=OSHA Z     15=TSCA 12b  20=IL RTK        25=PA RTK
                                                        26=RI RTK

* EPA recently added new chemical substances to its TSCA Section 4 test rules.  Please contact the supplier to confirm whether the ingredients in this product currently appear on a TSCA 4 or TSCA 12b list. 
Code key:CARC=Carcinogen; SUS=Suspected Carcinogen; REPRO=Reproductive

-------------------------------------------------------------------------- 
16. OTHER INFORMATION
-------------------------------------------------------------------------- 

USE: GEAR OIL

NOTE: PRODUCTS OF EXXON MOBIL CORPORATION AND ITS AFFILIATED COMPANIES
ARE NOT FORMULATED TO CONTAIN PCBS.

Health studies have shown that many hydrocarbons pose potential human
health risks which may vary from person to person. Information provided
on this MSDS reflects intended use. This product should not be used for
other applications. In any case, the following advice should be
considered:

INJECTION INJURY WARNING:  If product is injected into or under the skin,
or into any part of the body, regardless of the appearance of the wound
or its size, the individual should be evaluated immediately by a
physician as a surgical emergency.  Even though initial symptoms from
high pressure injection may be minimal or absent, early surgical
treatment within the first few hours may significantly reduce the
ultimate extent of injury.

INDUSTRIAL LABEL

Under normal conditions of intended use, this product does not pose a
risk to health.  Excessive exposure may result in eye, skin or
respiratory irritation.  Always observe good hygiene measures.  First
Aid: Wash skin with soap and water.  Flush eyes with water.  If
overcome by fumes or vapor, remove to fresh air.  If ingested do not
induce vomiting.  If symptoms persist seek medical assistance.  Read
and understand the MSDS before using this product.

*************************************************************************
For Internal Use Only:  MHC:  1* 1* 1* 1* 1*, MPPEC:  A, TRN:  511121-44,
CMCS97:  973296, REQ:  CHILE, SAFE USE:  L
EHS Approval Date: 21MAY2003
*************************************************************************

Information given herein is offered in good faith as accurate, but
without guarantee. Conditions of use and suitability of the product for
particular uses are beyond our control; all risks of use of the product
are therefore assumed by the user and WE EXPRESSLY DISCLAIM ALL
WARRANTIES OF EVERY KIND AND NATURE, INCLUDING WARRANTIES OF
MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE IN RESPECT TO THE
USE OR SUITABILITY OF THE PRODUCT. Nothing is intended as a
recommendation for uses which infringe valid patents or as extending
license under valid patents. Appropriate warnings and safe handling
procedures should be provided to handlers and users. Alteration of this
document is strictly prohibited. Except to the extent required by law,
republication or retransmission of this document, in whole or in part, is
not permitted. Exxon Mobil Corporation and its affiliated companies
assume no responsibility for accuracy of information unless the document
is the most current available from an official ExxonMobil distribution
system. Exxon Mobil Corporation and its affiliated companies neither
represent nor warrant that the format, content or product formulas
contained in this document comply with the laws of any other country
except the United States of America.

Prepared by:  ExxonMobil Oil Corporation
     Environmental Health and Safety Department, Clinton, USA

<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd"><html xmlns="http://www.w3.org/1999/xhtml"><head><title></title></head><body>    <form name="form1" method="post" action="Download.aspx?ID=7722&amp;docFormat=RTF" id="form1"><div><input type="hidden" name="__VIEWSTATE" id="__VIEWSTATE" value="/wEPDwULLTE2MTY2ODcyMjlkZIJ5qID85+05PcQwqU1GdcFliVVN" /></div>    <div>        </div>    </form></body></html>